00000aaa # Test 5.3.1.5: readback value of MIE after enabling all interrupts.
00000222 # readback value of mideleg after attempting to delegate all interrupts.
0000000b # mcause from ecall for going from M mode to S mode
00000000 # mtval of ecall (*** defined to be zero for now)
00001800 # masked out mstatus.MPP = 11, mstatus.MPIE = 0, and mstatus.MIE = 0
80000001 # mcause from s soft interrupt
00000000 # mtval for ssoft interrupt (0x0)
00000120 # masked out sstatus.SPP = 1, sstatus.SPIE = 1, and sstatus.SIE = 0
00000009 # mcause from ecall for going from S mode to M mode
00000000 # mtval of ecall (*** defined to be zero for now)
00000800 # masked out mstatus.MPP = 01, mstatus.MPIE = 0, and mstatus.MIE = 0
0000000b # mcause from ecall for going from M mode to U mode
00000000 # mtval of ecall (*** defined to be zero for now)
00001800 # masked out mstatus.MPP = 11, mstatus.MPIE = 0, and mstatus.MIE = 0
80000001 # mcause from s soft interrupt from user mode this time
00000000 # mtval for mtime interrupt (0x0)
00000020 # masked out sstatus.SPP = 0, sstatus.SPIE = 1, and sstatus.SIE = 0
00000008 # mcause from U mode ecall from test termination
00000000 # mtval of ecall (*** defined to be zero for now)
00000000 # masked out mstatus.MPP = 00, mstatus.MPIE = 0, and mstatus.MIE = 0
