00000000 # msip zero on reset
00000000 # mip is zero
00000008 # mip msip bit is set
00000000 # mip msip bit is reset
00000000 # mip mtip bit is reset
FFFFFFFF # mtimecmp is same as written value
A5A5A5A5 # mtimecmph is same as written value
00000000 # mip mtip is zero
00000080 # mip mtip is set
