0000000b # test 5.3.1.6: mcause for ecall from going to S mode from M mode
00000000
00000000 # mtval of ecall (*** defined to be zero for now)
00000000
00001800 # masked out mstatus.MPP = 11, mstatus.MPIE = 0, and mstatus.MIE = 0
00000000
00000002 # mcause for illegal sret instruction due to status.tsr bit being set.
00000000
10200073 # mtval of illegal instruction (illegal instruction's machine code)
00000000
00000800 # masked out mstatus.MPP = 01, mstatus.MPIE = 0, and mstatus.MIE = 0
00000000
00000009 # mcause from S mode ecall from test termination
00000000
00000000 # mtval of ecall (*** defined to be zero for now)
00000000
00000800 # masked out mstatus.MPP = 01, mstatus.MPIE = 0, and mstatus.MIE = 0
00000000
