// Copyright lowRISC contributors.
// Licensed under the Apache License, Version 2.0, see LICENSE for details.
// SPDX-License-Identifier: Apache-2.0
{
  // Name of the sim cfg - typically same as the name of the DUT.
  name: prim_prince

  // Top level dut name (sv module).
  dut: prim_prince

  // Top level testbench name (sv module).
  tb: prim_prince_tb

  // Simulator used to sign off this block
  tool: vcs

  // Fusesoc core file used for building the file list.
  fusesoc_core: lowrisc:dv:prim_prince_sim:0.1

  // Import additional common sim cfg files.
  import_cfgs: ["{proj_root}/hw/dv/tools/dvsim/common_sim_cfg.hjson",
                // Config files to get the correct flags for crypto_dpi_prince
                "{proj_root}/hw/ip/prim/dv/prim_prince/crypto_dpi_prince/crypto_dpi_prince_sim_opts.hjson"]

  en_build_modes: ["{tool}_crypto_dpi_prince_build_opts"]

  // Default iterations for all tests - each test entry can override this.
  reseed: 50

  // Enable cdc instrumentation
  run_opts: ["+cdc_instrumentation_enabled=1"]

  overrides: [
    {
      name: vcs_cov_cfg_file
      value: "-cm_hier {proj_root}/hw/ip/prim/dv/prim_prince/data/prim_prince_cover.cfg"
    }
  ]

  // List of test specifications.
  tests: [
    {
      name: prim_prince_test
    }
  ]

  // List of regressions.
  regressions: [
    {
      name: smoke
      tests: ["prim_prince_test"]
    }
    {
      name: nightly
      // Run the same test as the "smoke" regression, just with a higher reseed value.
      // This higher reseed value is due to the rather large state space created by
      // the 128-bit key and 64-bit data values.
      reseed: 500
    }
  ]
}
